Rename the unforce_hd60.txt to force_hd60.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will force to install the image M46988_ax60_v2-03_stable_UPDATEUSB_g27073_multi.zip in the linux1 selection
