Rename the unforce_hd61.txt to force_hd61.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will force to install the image M47039_ax61_v2-04_stable_UPDATEUSB_g27321_multi.zip in the linux1 selection
